### Summary

Design Name | mdrive2
Fitting Status | Successful
Software Version | L.33
Device Used | XC9572-15-PC44
Date | 6-13-2012, 7:32PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
30/72 (42%) | 68/360 (19%) | 26/72 (37%) | 7/34 (21%) | 41/144 (29%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 2 | 2
Output | 4 | 4
Bidirectional | 0 | 0
GCK | 1 | 1
GTS | 0 | 0
GSR | 0 | 0
Pin Type | Used | Total
--- | --- | ---
I/O | 6 | 29
GCK/IO | 1 | 3
GTS/IO | 0 | 2
GSR/IO | 0 | 1

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | CLK

##### POWER DATA

Macrocells in high performance mode (MCHP) | 30
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 30